{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["报价单格式"],"not_rendered":{"images":17,"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"报价单格式","index":0,"n_rows":18,"n_cols":8,"rows_kept":18,"merged":[[0,0,0,7],[18,0,18,7],[21,2,21,3],[21,4,21,7]],"flags":["formulas_cached_only"]}
["采购清单"]
["序号","产品参考图示","产品名称","规       格","颜色","单位","数量","材料说明"]
["1",null,"大班台","2200*1100*760H","经典胡桃","张",2,"1、基材采用欧标E0级环保型中纤板/刨花板；2、面贴优质胡桃木皮；3、油漆采用“大宝”牌优质环保油漆；4、采用优质五金配件。"]
["2",null,"三门书柜","1200*345*1880H","经典胡桃","组",2,"1、基材采用欧标E0级环保型中纤板/刨花板；2、面贴优质胡桃木皮；3、油漆采用“大宝”牌优质环保油漆；4、采用优质五金配件。"]
["3",null,"班椅","620*720*1100H","红胡桃","张",7,"1、椅架采用优质实木，经烘干、除虫等处理；2、油漆采用“大宝”牌优质环保油漆；3、优质五金配件。"]
["4",null,"单人位沙发","930*870*850H","PU黑色/红胡桃","张",4,"1、面料采用优质环保皮皮，外观色泽均匀，自然，手感柔软；2、内部采用实木框架，填充高密度海绵，回弹力好；3、脚架采用优质实木制作，经干燥、脱脂、除虫处理；4、油漆采用“大宝”牌优质环保油漆。"]
["5",null,"方茶几","600*600*500H","经典胡桃","张",2,"1、基材采用欧标E0级环保型中纤板/刨花板；2、面贴优质胡桃木皮；3、油漆采用“大宝”牌优质环保油漆；4、采用优质五金配件。"]
["6",null,"GB829-181班台","1800*900*760H","经典胡桃","张",5,"1、基材采用欧标E0级环保型中纤板/刨花板；2、面贴优质胡桃木皮；3、油漆采用“大宝”牌优质环保油漆；4、采用优质五金配件。"]
["7",null,"双门书柜","800*345*1880H","经典胡桃","组",2,"1、基材采用欧标E0级环保型中纤板/刨花板；2、面贴优质胡桃木皮；3、油漆采用“大宝”牌优质环保油漆；4、采用优质五金配件。"]
["8",null,"办公桌","1400*700*760H","经典胡桃","张",40,"1、基材采用欧标E0级环保型中纤板/刨花板；2、面贴优质胡桃木皮；3、油漆采用“大宝”牌优质环保油漆；4、采用优质五金配件。"]
["9",null,"转椅","560*550*950-1030H","PU黑色/红胡桃","张",40,"1、采用优质环保皮，外观色泽均匀，自然，手感柔软；2、内部采用多层胶合板，填充高密度海绵；3、可升降转动气杆，采用原装气压棒，带前后倾仰同步锁止机构；4采用五星脚架，优质实木扶手及脚架，经干燥、脱脂、除虫处理；5、油漆采用“大宝”牌优质环保油漆；6、采用优质五金配件。"]
["10",null,"条形桌","1400*400*760H","经典胡桃","张",14,"1、基材采用欧标E0级环保型中纤板/刨花板；2、面贴优质胡桃木皮；3、油漆采用“大宝”牌优质环保油漆；4、采用优质五金配件。"]
["11",null,"会议椅","460*550*910H","红胡桃","张",40,"1、椅架采用优质实木，经烘干、除虫等处理；2、油漆采用“大宝”牌优质环保油漆；3、优质五金配件。"]
["12",null,"会议桌","3200*1500*760H","经典胡桃","张",1,"1、基材采用欧标E0级环保型中纤板/刨花板；2、面贴优质胡桃木皮；3、油漆采用“大宝”牌优质环保油漆；4、采用优质五金配件。"]
["13",null,"保密柜","850*390*1850H","灰白色","组",2,"采用优质冷轧钢板，钢板厚板为0.6mm，冲压成型；钢板表面经过碱洗除油、酸洗除锈、磷化附膜、钝化、静电机器手自动喷涂和高温固化处理。热固性粉末喷塑；除锈、耐磨、防腐蚀。符合GB/T3325-2008金属家具通用技术条件；灰白色。"]
["14",null,"五节档案柜","850*360*2060H","灰白色","组",37,"采用优质冷轧钢板，钢板厚板为0.6mm，冲压成型；钢板表面经过碱洗除油、酸洗除锈、磷化附膜、钝化、静电机器手自动喷涂和高温固化处理。热固性粉末喷塑；除锈、耐磨、防腐蚀。符合GB/T3325-2008金属家具通用技术条件；灰白色。"]
["15",null,"保险柜","460*420*800H","古铜色","个",1,"采用优质冷轧钢板，钢板厚板为0.6mm，冲压成型；钢板表面经过碱洗除油、酸洗除锈、磷化附膜、钝化、静电机器手自动喷涂和高温固化处理。热固性粉末喷塑；除锈、耐磨、防腐蚀。符合GB/T3325-2008金属家具通用技术条件；灰白色。"]
["16",null,"保险柜","400*350*530H","古铜色","个",1,"采用优质冷轧钢板，钢板厚板为0.6mm，冲压成型；钢板表面经过碱洗除油、酸洗除锈、磷化附膜、钝化、静电机器手自动喷涂和高温固化处理。热固性粉末喷塑；除锈、耐磨、防腐蚀。符合GB/T3325-2008金属家具通用技术条件；灰白色。"]